Squeezelite / Logitech Media Server

Squeezelite is a network music player which could be used with Logitech Media Server(aka. LMS). Eunhasu has LMS inside of itself which is available Tidal, Qobuz and internet radio.

Name: A name of device Squeezelite appearing on LMS. This could be changed if you need.

Audio device config: Select a radio button of USB DAC which is going to use and click ‘Save changes’ to use the USB DAC.

DSD mode: Set playback mode. Convert music to PCM or playing DSD music file by DoP or native. DAC should support native DSD when native mode.

Clear artwork.db: Delete LMS artwork database file. You should rescan in LMS to generate deleted file.

Clear config cache: Delete LMS config cache files.

Configuration

Check your DAC's capability.

Input 'Max samplerate' and 'Sample format' by DAC information. Please refer to highlighted part.

LMS library rescan guide

Move on to Settings menu page.

Click “Rescan” button to start scan on Basic Settings tab.

Click “Scanning - View Progress” link at bottom of page if you'd like to see scanning states.

Scanning states screen.

ickStream

ickStream plugin provides lots of third-party feature like Quboz, TIDAL. Install guide are following.

http://wiki.ickstream.com/index.php/Open_Beta_Squeezebox_Installation

After finish ickStream plugin installation, you have to agree EULA and login ickStream in LMS > Settings > Advanced > ickStream page.

Login complete.

You can see ickStream item in My Apps of LMS main screen.

Video: how to install and set Spotify plugin in LMS; Spotify premium account required.